The **ETsz()** instruction requires the user to input lattitude, longitude, elevation, and crop type for a station's location in order to generate accurate calculations of ET. The Generic\_ET\_107\_ETsz.CR1 and Generic\_ET\_107\_ETsz\_Windsonic.CR1 programs use the **ConstTable()** intruction to create a constants table that allows the user to easily input these values using Loggernet, PC400, or a keyboard display. Note: these values only need to be set once, during station set up.